***IS 456 COLUMN CODE PROVISIONS***

Column definition Column Effective Length > 3 x Minmum(b,d) **[IS 456 25.1.1]**

Short Column EffectiveLength(lx)/D < 12 and ly/b < 12 **[IS 456 25.1.2]**

Long Column EffectiveLength /D >= 12 or y/b >= 12  **[IS 456 25.1.2]**

Slenderness Limit

End Restrained: UnsupportedLength <= 60 x Minimum(b,d)  **[25.3.1]**

One end Unrestrained(cantilever): UnsupportedLength <= 100 b2 /D **[25.3.2]**

Minimum Eccentricity **[24.4]**

Min of below

UnsupportedLength(l)/500 + RespectiveLateralDimension(b,d)/30

20 mm

Cover Minimum Cover >= 40 **[Is 456 26.4.2.1]**

Min dimension >= 200 that is only for column

who have bars dia <=12 only and cover =25 can be use **[Is 456 26.4.2.1]**

Min Reinforcement **0.008 b d** (gross cross section) **[Is 456 26.5.3.1]**

Max Reinforcement **0.06 b d** (gross cross section) **[Is 456 26.5.3.1]**

**Minimum no of bars is [Is 456 26.5.3.1\_c]**

4 in Rectangular Column

6 in Circle Column

Min Bar diameter **dia >=12 mm [Is 456 26.5.3.1\_d]**

Max spacing of main bar **spacing <= 300 [Is 456 26.5.3.1\_h]**

**Lateral ties min spacing**  **[Is 456 26.5.3.2\_c]**

Min of below 3

Min (b,d)

16 Dia(longitutional)

300

**Dia of tie/Helical [Is 456 26.5.3.2\_d]**

Max of below :

¼ dia of large longitudinal bar

16

**Pitch of tie/Helical [Is 456 26.5.3.2\_d]**

Max pitch

Min of below

1/6 x Dia of column

75

Min pitch

Max of below

3 x Dia of helix bar

25

* Max Compressive Strain in concrete ‘Concrete in Compressive only’

**0.002 [Is 456 39.1]**

* Max Compressive Strain in concrete concrete ‘Concrete in Compressive and bending’ when there is no tension in the section

**0.0035 – 0.75 x strain in least compressive fibre [Is 456 39.1]**

**Short Axially Loaded Column**  **[Is 456 39.3]**

Le/b < 12 short column

UnsupportedLength(l)/500 + RespectiveLateralDimension(b,d)/30 <= 0.05 x Lateral Dimension <= 20

Pu = 0.4 fck Ac + 0.67 fy Asc

**Compression Members with Helical Reinforcement** **[Is 456 39.4]**

Pu = (0.4 fck Ac + 0.67 fy Asc ) x 1.05 of tie section

**Area of helical Reinforcenment** >= 0.36(Ag/Ac - 1) fkc/fy

**Members Subjected to Combined Axial Load and Biaxial Bending [Is 456 39.6]**


This ensure that this that member is with in the Circle or curve dose not fail

***= Pu/ Puz***

***Puz =*** 0.45fck Ac + 0.75 fy Asc  

**Slender compession members [39.7]**

Additional Moment



Reduction Factor **[39.7.1.1]**

**

Concrete Shear Capacity  **[40.4 c] [T table 19]**

***Shear Strength of Members Under axial [ 40.2.2]***

*Design shear strength of table119 must multiply with factor*

*Detla = 1 + 3 Pu / Ag fck*

***Tc*** *x Delta*

Design Shear Strength of Concrete ***Tc [Table 19]***


*Shear Strength of Concrete* ***Tc*** ***[sp 24 39.2.1]***

*Shear Strength of Concrete Tcmax*  *[Table 20 , sp 16 pno124]*

Reinforce Shear Capacity   **[40.4 c]**

Minimum shear reinforcement **[26.5.1.6]**

**Effective Length [ Annex E ]**


As PER Table 28 


**Serviceability for Compression Member [43.2]**

To considered flexural member for purpose of crack controle

Axial load **<=** 0.2 fck Ac

**Design surface Crack Width**  **[Annex F]**





**Cracking Limits** **[35.3.2]**

For Appearance Condition Crack Width Not Exceed 0.3 mm

For Moderate Exposer Condition Crack Width Not Exceed 0.2 mm

For Severe Exposer Condition Crack Width Not Exceed 0.1 mm

For Aggressive Condition Crack width not Exceed 0.004 mm

**Splicing**  **[26.5.5.1]**

Lap splices

Ø ≤ 36 mm

If ø ≥ 36 mm provide spirals around lapped bar

++

**Maximum Allowable Spacing of shear steel [26.5.1.5]**

Min of below

0.75 d

300

**Minimum****Distance between Individual Bars *[*26.3.2]**

Not greater than this :

Dia of Large Bar

5mm + 20aggregate size

Check ratio of tensile reinforcement

Calculate Neutral axis  **[ANNEX G]**

Calculate Moment Capacity  **[ANNEX G]**

Calculate Moment Capacity compression steel  **[ANNEX G 1-2]**

xu.max the limiting value of xU **xu.max**  **[38.1]**

***Stress in Compression Steel fsc*  [Annex G 1.2]**

***Xu / d Limit [Table 20 , sp 16 pno124]***

**IS 13920 DUCTAIL DETAILING [7]**

**Minimum Column width [7.1.1]**

**Max of Below**

>= 300

>= 20 Diameter\_Longitudinal\_Large\_bar

**Smaller\_section\_dimension to Larger\_section\_dimension <= 0.45 [7.1.2]**

b/d <=0.45

Circular column minimum of **6** bars **[7.3.1]**

**If Splicing [7.3.2.1]**

Link spacing <= 100 mm spacing

mainBar Dia <= 32 mm

Hook **135** degree and must extend 6 times its diameter and >=65 mm **[7.4.1]**

Show in Drawings

**Links spacing [7.4.2]**

Minimum bar Dia >= 8mm

Maximum bar Dia <= 32mm

If Dia of long bar is 32 mm then minimum bar dia <= 10

Max spacing links(TieBar) <= 300

Spacing<= ½ min(b,d)

If length of link is >= 300 provide cross link

**Shear Force in Columns** sagging-hogging [7.5]

For Sway to Right Vu = 1.4 (MuAs  + MuBh )/hst

For Sway to Left Vu = 1.4 (MuAh  + MuBs )/hst